**Contractor Stormwater Compliance Agreement**

**Construction and Building Maintenance Contractors:**

* Do not rinse or clean equipment or machines near stormwater catchbasins or near any stormwater conveyance system (for example: storm sewer, catchbasins, manholes, detention / retention basins, open drains, swales, established county drains, rivers, streams or lake or other natural surface water bodies such as wetlands.)
* Keep all materials from entering the site’s stormwater conveyance system.
* Prevent fuels, paints, solvents, cleaning fluids or any fluid other than clean water from spilling onto or into curbs / gutters, or stormwater systems or the conveyance systems mentioned above.
* Report any spills of polluting materials to the city/village immediately.
* If the construction site has disturbed the soils in an area of one acre or more or is within 500 feet of waters of the state, including a county drain, the contractor must have a MDEQ certified storm water operator in the work crew on site.

I have read and understand the above items and will make every effort not to create a situation that may cause the impairment of stormwater on this site. I ensure to perform all municipal operation and maintenance activities so they comply with all pollution prevention and good housekeeping Best Management Practices (BMPs) as deemed appropriate. This information will be communicated to our employees and I take responsibility for their actions.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature Date

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Printed Name

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Organization